

**The Sunshade Sandbox**



**LIST OF MATERIALS**   
(finished dimensions in inches)

|  |  |  |
| --- | --- | --- |
| A | Sides (4) | 3/4 x 7-1/4 x 47-1/4 |
| B | Posts (2) | 3-1/2 x 3-1/2 x 48 |
| C | Seats (cut two diagonally from) | 3/4 x 11-1/4 x 11-1/4 |
| D | Shelf (1) | 3/4 x 7-1/4 x 46-1/2 |
| E | Shelf Back (1) | 3/4 x 5-1/4 x 46-1/2 |
| F | Pivot supports (2) | 1/2 x 7-1/8 x 12 |
| G | Canopy sides(2) | 3/4 x 2-1/4 x 48 |
| H | Canopy ends (2) | 3/4 x 3-3/4 x 37 |
| J | Bottom (1) (plywood) | 1/2 x 46-1/2 x 46-1/2 |
| K | Cover (1) (plywood) | 1/4 x 48 x 48 |
| L | Cleat strips (21) | 3/4 x 3/4 x various |
| M | Dowel rods (2) | 3/4 dia. x 36 |
| N | Sun shade (canvas) | 36 x 60 |
|  | | |
| **HARDWARE** | | |
| (2) | 3/8 "- 16 x 5" long carriage bolts | |
| (2) | 3/8 "- 16 x 6" long roundhead stove bolts | |
| (6) | 3/8" I.D. fender washers | |
| (2) | 1/2" I.D. fender washers | |
| (2) | 3/8" I.D. flat washers | |
| (4) | 3/8" - 16 hex nuts | |
| (2) | 3/8" - 16 wing nuts | |
| (8) | 5/16" I.D. flat washers | |
| (8) | 5/16" x 3" lag screws | |
| (32) | #6 x 1" drywall screws | |
| (5) | #6 x 1-1/4" drywall screws | |
| (4) | #6 x 1-1/2" drywall screws | |
|  | 1/2# 4-penny finishing nails | |

**View Plans &   
Assembly Drawings**[Assembly](http://www.shopsmithhandson.com/archives/july_aug_02/html/weekendproject/wp_plans1.htm)   
[Bottom Layout](http://www.shopsmithhandson.com/archives/july_aug_02/html/weekendproject/wp_plans2.htm)[Cover Layout](http://www.shopsmithhandson.com/archives/july_aug_02/html/weekendproject/wp_plans3.htm)